|  |  |  |
| --- | --- | --- |
| **Pos.** | **Description** | **Quantity** |
| 1. | Single Mode Wide Band Coupler, Grade P, 1060nm, 20/80, 2x2, Package B, 2m of 900um Jacket, HI1060, 4 FC/APC Connectors Fyber Type: WP10200202B2111-2m http://www.acphotonics.com/products/Product%20files/Fused%20Coupler/Singlemode%20Fiber%20Coupler.htm | 3 |
| 2. | Single Mode Wide Band Coupler, Grade P, 1060nm, 30/70, 2x2, Package B, 2m of 900um Jacket, HI1060, 4 FC/APC Connectors Fiber type: WP10300202B2111-2m http://www.acphotonics.com/products/Product%20files/Fused%20Coupler/Singlemode%20Fiber%20Coupler.htm | 3 |
| 3. | Single Mode Wide Band Coupler, Grade P, 1060nm, 50/50, 2x2, Package B, 2m of 900um Jacket, HI1060, 4 FC/APC Connectors Fiber type: WP10500202B2111-2m http://www.acphotonics.com/products/Product%20files/Fused%20Coupler/Singlemode%20Fiber%20Coupler.htm | 3 |
| 4. | Single Mode Wide Band Coupler, Grade P, 1060nm, 10/90, 2x2, Package B, 2m of 900um Jacket, HI1060, 4 FC/APC Connectors Fiber type: WP10100202B2111-2m http://www.acphotonics.com/products/Product%20files/Fused%20Coupler/Singlemode%20Fiber%20Coupler.htm | 2 |
| 5. | Single Mode Patch Cord, FC/APC Connector to FC/APC Conn., Simplex (1 Core), HI1060, 2m on Fiber Length Fiber type: PSFA1FA1102 | 1 |

*Chancellor*

*MA Justyna Morzy*